**Skypark Arriving and Departing**

1. **KBTF Arrivals:**
   * Remain East of airport to avoid SLC Class B airspace
   * Useable KBTF Runway 4600 ft

IFR Weather:

* Follow SLC Approach path to Break off When KBTF in sight

VFR Weather:

* ATC request that you cancel IFR outside of SLC Class B airspace
  + South of FFU (Fairfield VOR)
  + North of OGD (Ogden VOR)

Please be familiar with SLC Class B airspace.

1. **KBTF Departures:**


**VFR Departures used**

* Shoreline:
  + VPLGN (lagoon Amusement Park) then northwest along shoreline
  + Stay below SLC Class B or obtain Bravo Clearance
* Mountain Road:
  + VPLGN (Lagoon Amusement Park)
  + Climb North along the mountain road
  + NOTE: Be familiar with Class B airspace
* Southbound:
  + Remain East and clear of Class B airspace, or
  + Contact SLC Tower on 120.2 for Class B Transition

Please be familiar with SLC Class B airspace.

**IFR Departures:**

* + SL TRACON Flow Control: 801-325-9672
  + SL Clearance Delivery on 120.7

Runway 17-35 Takeoff Procedures

DO NOT USE TAKOFF POWER UNTIL PAST YELLOW TRESHOLD